{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Well 1 (WM)","Well 2 (SM)","Ref Well","lists","Well Illustration"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Well 1 (WM)","index":0,"n_rows":22,"n_cols":13,"rows_kept":22,"cut":false,"hidden":false,"merged":[[16,5,16,7],[16,8,16,10],[17,3,17,4],[12,0,12,3],[12,4,12,11],[13,0,13,3],[13,4,13,11],[14,0,14,1],[14,2,14,12],[10,0,10,2],[10,5,10,7],[10,8,10,10],[11,0,11,2],[11,5,11,7],[11,8,11,10],[8,0,8,2],[8,5,8,7],[8,8,8,10],[9,0,9,2],[9,5,9,7],[9,8,9,10],[5,11,5,12],[6,0,6,3],[6,4,6,8],[6,9,6,11],[7,0,7,3],[7,4,7,8],[7,9,7,11],[4,0,4,1],[4,5,4,6],[4,7,4,8],[4,9,4,10],[5,5,5,6],[5,7,5,8],[5,9,5,10],[0,0,0,12],[1,0,1,12],[2,0,2,1],[2,5,2,8],[2,9,2,10],[2,11,3,11],[2,12,3,12],[3,0,3,3],[3,5,3,8],[3,9,3,10]]}
["Minnesota Board of Water & Soil Resources"]
["Soil Boring/ Well Construction Log"]
["Project:",null,null,null,"Site ID","County",null,null,null,"Date",null,"Boring/ Well No.","Well 1"]
["Madsen Wetland Bank",null,null,null,"s08907","Lincoln",null,null,null,"2021-04-20"]
["Location:",null,null,"UTM (m) X:","UTM (m) Y:","T",null,"Range",null,"Sec",null,"Personnel:"]
["E side - Wet 1 (WM)",null,null,-96.134658999999999,44.219718,"109N",null,"44W",null,27,null,"B Carlson"]
["Landscape Position",null,null,null,"Soil Series",null,null,null,null,"Parent Material",null,null,"Equipment/Method"]
["Concave slope, 1%",null,null,null,"Lakepark complex",null,null,null,null,"loamy colluvium over glacial\ntill",null,null,"Dutch Auger"]
["Screen Type",null,null,"Screen Length","Diameter","Slot Size",null,null,"Screen Interval",null,null,"Pack Interval","Pack Material"]
["Sch 40 PVC, wrap",null,null,2.4500000000000002,"1.25 in.",0.01,null,null,"0.5 - 2.4",null,null,"0.5 - 3.3","sand"]
["Riser Type",null,null,"Riser Length","Total Length","Stick up",null,null,"Depth",null,null,"End Plug","Backfill Material"]
["Sch 40 PVC",null,null,3.05,5.5,2.2200000000000002,null,null,{"$f":"+E12-F12","v":3.28},null,null,"vented cap","native soil/bentonite"]
["Seal(s)",null,null,null,"Surface Completion",null,null,null,null,null,null,null,"Initial Water Level"]
["Bentonite",null,null,null,"oversize PVC cap",null,null,null,null,null,null,null,"-1.78'"]
["Installation Notes: ",null,"Initial water level after 1 hour"]
[]
["thick","from","to ",null,null,"Matrix",null,null,"Redox"]
["(ft)","(ft)","(ft)","texture",null,"%","H","V/C","%","H","V/C","Remarks","Well"]
[{"$f":"+F12","v":2.2200000000000002},-1.5,0,"ground surface",null,null,null,null,null,null,null,"2.22' stickup"]
[{"$f":"+C20-B20","v":1.5},0,1.5,"Clay Loam",null,1,"10YR","2/1"]
[1.83,1.5,3.33,"Sandy Clay Loam",null,1,"10YR","2/1"]
[null,null,null,"end of boring"]

{"sheet":"Well 2 (SM)","index":1,"n_rows":22,"n_cols":13,"rows_kept":22,"cut":false,"hidden":false,"merged":[[0,0,0,12],[1,0,1,12],[2,0,2,1],[2,5,2,8],[2,9,2,10],[2,11,3,11],[2,12,3,12],[3,0,3,3],[3,5,3,8],[3,9,3,10],[4,0,4,1],[4,5,4,6],[4,7,4,8],[4,9,4,10],[5,5,5,6],[5,7,5,8],[5,9,5,10],[5,11,5,12],[6,0,6,3],[6,4,6,8],[6,9,6,11],[7,0,7,3],[7,4,7,8],[7,9,7,11],[8,0,8,2],[8,5,8,7],[8,8,8,10],[9,0,9,2],[9,5,9,7],[9,8,9,10],[10,0,10,2],[10,5,10,7],[10,8,10,10],[11,0,11,2],[11,5,11,7],[11,8,11,10],[16,5,16,7],[16,8,16,10],[17,3,17,4],[12,0,12,3],[12,4,12,11],[13,0,13,3],[13,4,13,11],[14,0,14,1],[14,2,14,12]]}
["Minnesota Board of Water & Soil Resources"]
["Soil Boring/ Well Construction Log"]
["Project:",null,null,null,"Site ID","County",null,null,null,"Date",null,"Boring/ Well No.","Well 2"]
["Madsen Wetland Bank",null,null,null,"s08907","Lincoln",null,null,null,"2021-04-20"]
["Location:",null,null,"UTM (m) X:","UTM (m) Y:","T",null,"Range",null,"Sec",null,"Personnel:"]
["W side - Wet 1 (SM)",null,null,-96.141841999999997,44.220559999999999,"109N",null,"44W",null,28,null,"B Carlson"]
["Landscape Position",null,null,null,"Soil Series",null,null,null,null,"Parent Material",null,null,"Equipment/Method"]
["Concave basin, < 1%",null,null,null,"Rauville silty clay loam",null,null,null,null,"alluvium on floodplains\ntill",null,null,"Dutch Auger"]
["Screen Type",null,null,"Screen Length","Diameter","Slot Size",null,null,"Screen Interval",null,null,"Pack Interval","Pack Material"]
["Sch 40 PVC, wrap",null,null,2.5,"1.25 in.",0.01,null,null,"0.5 - 2.5",null,null,"0.5 - 2.85","sand"]
["Riser Type",null,null,"Riser Length","Total Length","Stick up",null,null,"Depth",null,null,"End Plug","Backfill Material"]
["Sch 40 PVC",null,null,3.62,6.15,3.3,null,null,{"$f":"+E12-F12","v":2.8500000000000005},null,null,"vented cap","native soil/bentonite"]
["Seal(s)",null,null,null,"Surface Completion",null,null,null,null,null,null,null,"Initial Water Level"]
["Bentonite",null,null,null,"oversize PVC cap",null,null,null,null,null,null,null,"+0.25'"]
["Installation Notes: ",null,"Installed in standing water"]
[]
["thick","from","to ",null,null,"Matrix",null,null,"Redox"]
["(ft)","(ft)","(ft)","texture",null,"%","H","V/C","%","H","V/C","Remarks","Well"]
[{"$f":"+F12","v":3.3},-1.5,0,"ground surface",null,null,null,null,null,null,null,"3.3' stickup"]
[3,0,3,"Clay Loam",null,1,"10YR","2/1"]
[]
[null,null,null,"end of boring"]

{"sheet":"Ref Well","index":2,"n_rows":23,"n_cols":13,"rows_kept":23,"cut":false,"hidden":false,"merged":[[0,0,0,12],[1,0,1,12],[2,0,2,1],[2,5,2,8],[2,9,2,10],[2,11,3,11],[2,12,3,12],[3,0,3,3],[3,5,3,8],[3,9,3,10],[4,0,4,1],[4,5,4,6],[4,7,4,8],[4,9,4,10],[5,5,5,6],[5,7,5,8],[5,9,5,10],[5,11,5,12],[6,0,6,3],[6,4,6,8],[6,9,6,11],[7,0,7,3],[7,4,7,8],[7,9,7,11],[8,0,8,2],[8,5,8,7],[8,8,8,10],[9,0,9,2],[9,5,9,7],[9,8,9,10],[10,0,10,2],[10,5,10,7],[10,8,10,10],[11,0,11,2],[11,5,11,7],[11,8,11,10],[16,5,16,7],[16,8,16,10],[17,3,17,4],[12,0,12,3],[12,4,12,11],[13,0,13,3],[13,4,13,11],[14,0,14,1],[14,2,14,12]]}
["Minnesota Board of Water & Soil Resources"]
["Soil Boring/ Well Construction Log"]
["Project:",null,null,null,"Site ID","County",null,null,null,"Date",null,"Boring/ Well No.","Reference"]
["Madsen Wetland Bank",null,null,null,"s08907","Lincoln",null,null,null,"2021-04-20"]
["Location:",null,null,"UTM (m) X:","UTM (m) Y:","T",null,"Range",null,"Sec",null,"Personnel:"]
["Reference wetland",null,null,-96.155682999999996,44.273997000000001,"109N",null,"44W",null,4,null,"B Carlson"]
["Landscape Position",null,null,null,"Soil Series",null,null,null,null,"Parent Material",null,null,"Equipment/Method"]
["Concave basin, 1%",null,null,null,"Bigstone silt loam",null,null,null,null,"alluvium on till plains\ntill",null,null,"Dutch Auger"]
["Screen Type",null,null,"Screen Length","Diameter","Slot Size",null,null,"Screen Interval",null,null,"Pack Interval","Pack Material"]
["Sch 40 PVC, wrap",null,null,2.23,"1.25 in.",0.01,null,null,"0.5 - 2.2",null,null,"0.5 - 3.0","sand"]
["Riser Type",null,null,"Riser Length","Total Length","Stick up",null,null,"Depth",null,null,"End Plug","Backfill Material"]
["Sch 40 PVC",null,null,3.72,5.95,2.92,null,null,{"$f":"+E12-F12","v":3.0300000000000002},null,null,"vented cap","native soil/bentonite"]
["Seal(s)",null,null,null,"Surface Completion",null,null,null,null,null,null,null,"Initial Water Level"]
["Bentonite",null,null,null,"oversize PVC cap",null,null,null,null,null,null,null,"-0.02'"]
["Installation Notes: ",null,"H2O at surface"]
[]
["thick","from","to ",null,null,"Matrix",null,null,"Redox"]
["(ft)","(ft)","(ft)","texture",null,"%","H","V/C","%","H","V/C","Remarks","Well"]
[{"$f":"+F12","v":2.92},-1.5,0,"ground surface",null,null,null,null,null,null,null,"2.92' stickup"]
[1.5,0,1.5,"Clay Loam",null,1,"N","2.5/0"]
[1,1.5,2.5,"Sandy Clay Loam",null,1,"N","2.5/0"]
[0.5,2.5,3,"Clay Loam",null,0.95,"10YR","4/1",0.05,"10YR","4/6"]
[null,null,null,"end of boring"]

{"sheet":"lists","index":3,"n_rows":87,"n_cols":15,"rows_kept":87,"cut":false,"hidden":false,"merged":[]}
["Gravel",null,null,null,null,null,null,null,null,null,null,null,"Aitkin","AITK",1]
["Coarse Sand","cos","COS",null,null,null,null,null,null,null,null,null,"Anoka","ANOK",3]
["Sand","s","S",null,null,null,null,null,null,null,null,null,"Becker","BECK",5]
["Fine Sand","fs","FS",null,null,null,null,null,null,null,null,null,"Beltrami","BELT",7]
["Very Fine Sand","vfs","VFS",null,null,null,null,null,null,null,null,null,"Benton","BENT",9]
["Loamy Coarse Sand","lcos","LCOS",null,null,null,null,null,null,null,null,null,"Big Stone","BIGS",11]
["Loamy Sand","ls","LS",null,null,null,null,null,null,null,null,null,"Blue Earth","BLUE",13]
["Loamy Fine Sand","lfs","LFS",null,null,null,null,null,null,null,null,null,"Brown","BROW",15]
["Loamy Very Fine Sand","lvfs","LVFS",null,null,null,null,null,null,null,null,null,"Carlton","CARL",17]
["Coarse Sandy Loam","cosl","COSL",null,null,null,null,null,null,null,null,null,"Carver","CARV",19]
["Sandy Loam","sl","SL",null,null,null,null,null,null,null,null,null,"Cass","CASS",21]
["Fine Sandy Loam","fsl","FSL",null,null,null,null,null,null,null,null,null,"Chippewa","CHIP",23]
["Very Fine Sandy Loam","vfsl","VFSL",null,null,null,null,null,null,null,null,null,"Chisago","CHIS",25]
["Loam","l","L",null,null,null,null,null,null,null,null,null,"Clay","CLAY",27]
["Silt Loam","sil","SIL",null,null,null,null,null,null,null,null,null,"Clearwater","CLEA",29]
["Silt","si","SI",null,null,null,null,null,null,null,null,null,"Cook","COOK",31]
["Sandy Clay Loam","scl","SCL",null,null,null,null,null,null,null,null,null,"Cottonwood","COTT",33]
["Clay Loam","cl","CL",null,null,null,null,null,null,null,null,null,"Crow Wing","CROW",35]
["Silty Clay Loam","sicl","SICL",null,null,null,null,null,null,null,null,null,"Dakota","DAKO",37]
["Sandy Clay","sc","SC",null,null,null,null,null,null,null,null,null,"Dodge","DODG",39]
["Silty Clay","sic","SIC",null,null,null,null,null,null,null,null,null,"Douglas","DOUG",41]
["Clay","c","C",null,null,null,null,null,null,null,null,null,"Faribault","FARI",43]
["Peat",null,null,null,null,null,null,null,null,null,null,null,"Fillmore","FILL",45]
["Muck",null,null,null,null,null,null,null,null,null,null,null,"Freeborn","FREE",47]
["Mucky Peat",null,null,null,null,null,null,null,null,null,null,null,"Goodhue","GOOD",49]
["Fibric Peat",null,null,null,null,null,null,null,null,null,null,null,"Grant","GRAN",51]
["Hemic Peat",null,null,null,null,null,null,null,null,null,null,null,"Hennepin","HENN",53]
["Sapric Peat",null,null,null,null,null,null,null,null,null,null,null,"Houston","HOUS",55]
[null,null,null,null,null,null,null,null,null,null,null,null,"Hubbard","HUBB",57]
["end of boring",null,null,null,null,null,null,null,null,null,null,null,"Isanti","ISAN",59]
[null,null,null,null,null,null,null,null,null,null,null,null,"Itasca","ITAS",61]
["summit",null,null,null,null,null,null,null,null,null,null,null,"Jackson","JACK",63]
["shoulder",null,null,null,null,null,null,null,null,null,null,null,"Kanabec","KANA",65]
["backslope",null,null,null,null,null,null,null,null,null,null,null,"Kandiyohi","KAND",67]
["footslope",null,null,null,null,null,null,null,null,null,null,null,"Kittson","KITT",69]
["toeslope",null,null,null,null,null,null,null,null,null,null,null,"Koochiching","KOOC",71]
[null,null,null,null,null,null,null,null,null,null,null,null,"Lac Qui Parle","LACQ",73]
[null,null,null,null,null,null,null,null,null,null,null,null,"Lake","LAKE",75]
[null,null,null,null,null,null,null,null,null,null,null,null,"Lake of the Woods","LOTW",77]
[null,null,null,null,null,null,null,null,null,null,null,null,"Le Sueur","LESU",79]
[null,null,null,null,null,null,null,null,null,null,null,null,"Lincoln","LINC",81]
[null,null,null,null,null,null,null,null,null,null,null,null,"Lyon","LYON",83]
[null,null,null,null,null,null,null,null,null,null,null,null,"Mahnomen","MAHN",87]
[null,null,null,null,null,null,null,null,null,null,null,null,"Marshall","MARS",89]
[null,null,null,null,null,null,null,null,null,null,null,null,"Martin","MART",91]
[null,null,null,null,null,null,null,null,null,null,null,null,"McLeod","MCLE",85]
[null,null,null,null,null,null,null,null,null,null,null,null,"Meeker","MEEK",93]
[null,null,null,null,null,null,null,null,null,null,null,null,"Mille Lacs","MILL",95]
[null,null,null,null,null,null,null,null,null,null,null,null,"Morrison","MORR",97]
[null,null,null,null,null,null,null,null,null,null,null,null,"Mower","MOWE",99]
[null,null,null,null,null,null,null,null,null,null,null,null,"Murray","MURR",101]
[null,null,null,null,null,null,null,null,null,null,null,null,"Nicollet","NICO",103]
[null,null,null,null,null,null,null,null,null,null,null,null,"Nobles","NOBL",105]
[null,null,null,null,null,null,null,null,null,null,null,null,"Norman","NORM",107]
[null,null,null,null,null,null,null,null,null,null,null,null,"Olmsted","OLMS",109]
[null,null,null,null,null,null,null,null,null,null,null,null,"Otter Tail","OTTE",111]
[null,null,null,null,null,null,null,null,null,null,null,null,"Pennington","PENN",113]
[null,null,null,null,null,null,null,null,null,null,null,null,"Pine","PINE",115]
[null,null,null,null,null,null,null,null,null,null,null,null,"Pipestone","PIPE",117]
[null,null,null,null,null,null,null,null,null,null,null,null,"Polk","POLK",119]
[null,null,null,null,null,null,null,null,null,null,null,null,"Pope","POPE",121]
[null,null,null,null,null,null,null,null,null,null,null,null,"Ramsey","RAMS",123]
[null,null,null,null,null,null,null,null,null,null,null,null,"Red Lake","REDL",125]
[null,null,null,null,null,null,null,null,null,null,null,null,"Redwood","REDW",127]
[null,null,null,null,null,null,null,null,null,null,null,null,"Renville","RENV",129]
[null,null,null,null,null,null,null,null,null,null,null,null,"Rice","RICE",131]
[null,null,null,null,null,null,null,null,null,null,null,null,"Rock","ROCK",133]
[null,null,null,null,null,null,null,null,null,null,null,null,"Roseau","ROSE",135]
[null,null,null,null,null,null,null,null,null,null,null,null,"Scott","SCOT",139]
[null,null,null,null,null,null,null,null,null,null,null,null,"Sherburne","SHER",141]
[null,null,null,null,null,null,null,null,null,null,null,null,"Sibley","SIBL",143]
[null,null,null,null,null,null,null,null,null,null,null,null,"St. Louis","STLO",137]
[null,null,null,null,null,null,null,null,null,null,null,null,"Stearns","STEA",145]
[null,null,null,null,null,null,null,null,null,null,null,null,"Steele","STEE",147]
[null,null,null,null,null,null,null,null,null,null,null,null,"Stevens","STEV",149]
[null,null,null,null,null,null,null,null,null,null,null,null,"Swift","SWIF",151]
[null,null,null,null,null,null,null,null,null,null,null,null,"Todd","TODD",153]
[null,null,null,null,null,null,null,null,null,null,null,null,"Traverse","TRAV",155]
[null,null,null,null,null,null,null,null,null,null,null,null,"Wabasha","WABA",157]
[null,null,null,null,null,null,null,null,null,null,null,null,"Wadena","WADE",159]
[null,null,null,null,null,null,null,null,null,null,null,null,"Waseca","WASE",161]
[null,null,null,null,null,null,null,null,null,null,null,null,"Washington","WASH",163]
[null,null,null,null,null,null,null,null,null,null,null,null,"Watonwan","WATO",165]
[null,null,null,null,null,null,null,null,null,null,null,null,"Wilkin","WILK",167]
[null,null,null,null,null,null,null,null,null,null,null,null,"Winona","WINO",169]
[null,null,null,null,null,null,null,null,null,null,null,null,"Wright","WRIG",171]
[null,null,null,null,null,null,null,null,null,null,null,null,"Yellow Medicine","YELL",173]

{"sheet":"Well Illustration","index":4,"n_rows":10,"n_cols":1,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
[1.5]
[1]
[1]
[1]
[1]
[1]
[1]
[1]
[1]
[1]